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PLAN A ASSESSMENT



Trainee Name:                                                                     Date of Assessment: 	       		  

Evaluator Conducting Assessment:                                          Location: 				                            

Evaluator: Conduct the assessment for one trainee at a time.  Do not give the trainee the answers or lead him/her in any way.  The assessment should be conducted in a quiet and un-rushed environment if possible.  Do not conduct the assessment prior to the end of the 30-day period, but as close as possible to the 30-day period (not more than 5 days later).  Correct the trainee during the evaluation process and demonstrate the correct method (if applicable).  Record performance on this evaluation sheet.

	Properties & Characteristics of Natural Gas
	Trainee
Passed
	
	Trainee
Failed

	Ask the trainee the following questions about Natural Gas
	
	
	

	1) What is the flammability range of natural gas?
	
	
	

	Answer:  5 – 15%
	
	
	

	2) What is the combustion by-product of natural gas?
	
	
	

	Score:   CO2 
	
	
	

	3) What is mercaptan and why is it important?
	
	
	

	Score:  It is the additive to natural gas to make it smell.  Without mercaptan gas is odorless, and a gas leak could be much more severe/deadly before detection.

	
	
	

	4) What is LEL and UEL?  What do these mean?
	
	
	

	Score: Lower Explosive Limit and Upper Explosive Limit.
	
	
	

	

5) Explain low, medium, and high pressure.  How do you identify? Adjust the question to fit your company.
	
	
	

	Score: Provides correct information about various pressures based on Company.
	
	
	




	 Proper Safety Equipment & Concerns Regarding Surroundings 
	Trainee
Passed
	
	Trainee
Failed

	Tell the trainee the following:  I’m going to give you a number of different situations that you would encounter on the job.  Please tell me what PPE you would wear or use in each.
	
	
	

	1) What PPE would you wear when cutting and threading pipe?
	
	
	

	Answer: Safety glasses, cut-proof gloves, hard hat, steel toed boots

	
	
	

	2) What about when working around blowing gas?
	
	
	

	Answer: Score based on your Company’s standards.

	
	
	

	3) What are your major concerns when working a job in a high traffic neighborhood? 
	
	
	

	Answer: Keeping an eye on traffic, possible bystanders, etc.
	
	
	

	4) In what situation would you use your breathing equipment? 
	
	
	

	Answer: Anytime gas is blowing
	
	
	

	5) What is the proper procedure if there is a fire?  
	
	
	

	Answer: Have the fire extinguisher present. Wear fire retardant clothing
	
	
	



	Tools, Equipment & Material
	Trainee
Passed
	
	Trainee
Failed

	Place most of the tools and equipment mentioned in the Plan A Tools & Equipment list on a table or make it available in the area of the testing (being certain to include all the tools and equipment needed to complete the assessment). Then ask the following questions or instruct the Trainee to do the following and record whether he/she passed or failed.  
	
	
	

	1) Point to a closed valve for which a valve wrench is the appropriate tool to open and ask: If I asked you to open this valve, what tool including what size would you use? 
	
	
	

	Score: Indicates the correct size Valve Wrench
	
	
	

	2) Put this ball valve on this pipe 
	
	
	

	Score: Should use Channel Locks or appropriate Pipe Wrench or Crescent Wrench properly
	
	
	

	3) Put this elbow on this piece of 3” pipe
	
	
	

	Score: Should use a Pipe Wrench properly
	
	
	

	4) Take this nut off the bolt and then put it back on
	
	
	

	Score: Should use a Socket Wrench properly
	
	
	

	
5) Make a ¼” hole in this steel plate
	
	
	

	Score:  Should use a drill press properly with the appropriate size bit
	
	
	

	6) Cut 3¼” off this piece of pipe 
	
	
	

	Score: Uses the Band Saw correctly
	
	
	

	
	
	
	

	Score: Pipe is cut to correct length
	
	
	

	7) Please check the _____________ area for a leak.
	
	
	

	Score: Trainee correctly uses the leak detection equipment to check the designated area for a leak.
	
	
	

	8) Perform a cadweld/exothermoweld on this piece of pipe to bond this tracer wire to the pipe.
	
	
	

	Score: Trainee cleans the pipe, correctly bonds the wire, and the cadweld/exothermoweld sticks.
	
	
	

	Provide the Trainee with the tape measuring questions.  Give the Trainee the following instructions: I am providing you with drawings of a tape measure. I want you to assume that the dark mark on each drawing is the amount you must measure for each item. You’ll notice that for each item you’ve been given four optional answers.  One of these is the correct answer.   
	
	
	

	9) b. 14-3/4”
	
	
	

	
	
	
	

	10)  d.  30-5/8”
	
	
	

	
	
	
	

	11)  a. 23-5/8”
	
	
	

	
	
	
	

	12)  a. 49-7/8”
	
	
	

	
	
	
	

	13)  d. 20-5/8”
	
	
	

	
	
	
	

	
	
	
	

	14)  c. 31-1/8”
	
	
	

	
	
	
	

	15)  b. 23-3/4”
	
	
	

	
	
	
	

	16)  a. 44-3/8”
	
	
	

	
	
	
	

	17)  d. 61-1/2”
	
	
	

	
	
	
	

	18)  a. 15-1/8”
	
	
	

	
	
	
	







	Types & Sizes of Pipes & Fittings
	Trainee
Passed
	
	Trainee
Failed

	Ask the following questions:
	
	
	

	1) Bring me a 1” 90 and a piece of 1” steel pipe 
	
	
	

		Score: Trainee does what was requested.
	
	
	

	2) Bring me a ¾ tee and a piece of ¾ PE pipe
	
	
	

	Score: Trainee does what was requested.
	
	
	

	3) Bring me a ¾” EFV
	
	
	

		Score: Trainee does what was requested.
	
	
	

	4) Name the most common fittings that go on service lines
	
	
	

		Score: (Must say all but regulator)
· Valve
· Riser
· Tapping tee
· Flow valve
· Pipe and wire
· Regulator
	
	
	

	5) Bring me a ¾” female steel to poly Mueller transition 
	
	
	

	Score: Trainee does what was requested.
	
	
	





	Gauges
	Trainee
Passed
	
	Trainee
Failed

	1) Pressure test this pipe to one and a half times 30 lbs. psi

	
	
	

	Score: Does as requested. Zeroes out the gauge. 

	
	
	

	2) Show me how you know that this is within calibration. 
	
	
	

	Score: Demonstrates that the gauge is correctly calibrated
	
	
	

	3) Bring me a low pressure gauge.
	
	
	

	Score: Does as requested.
	
	
	

	4) Bring me a high pressure gauge.
	
	
	

	Score: Does as requested.
	
	
	

	
5) When would you use a low pressure gauge and when would you use a high pressure gauge?
	
	
	

	Score: High pressure – pressure testing or setting pressure on higher pressure main.   Low pressure – service.
	
	
	




	Conducting a Soap Test
	Trainee
Passed
	
	Trainee
Failed

	Instruct the trainee to do the following
	
	
	

	1) Conduct a soap test on this pipe  
	
	
	

	Score: Trainee does what is requested  
	
	
	


	Utility Colors  
	Trainee
Passed
	
	Trainee
Failed

	Ask the trainee the following: Tell me what utilities the following colors represent. 
	
	
	

	1) Yellow
	
	
	

	Score: Gas, Hydrogen, Oil
	
	
	

	2) Orange
	
	
	

	Score: Fiber, Phone, Telecommunication
	
	
	

	3) Red
	
	
	

	Score: Power
	
	
	

	4) Green
	
	
	

	Score: Sewer
	
	
	

	5) Blue
	
	
	

	Score: Water
	
	
	

	6) White 
	
	
	

	Score: Proposed Digging/Work Area
	
	
	

	7) Pink
	
	
	

	Score: Survey
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